#!/bin/bash

source ~/.config.env

if [ ! "$MCONNECT" = true ] ; then
  echo "^c#EBCB8B^ ^d^"
  exit 0
fi

device_status=$(mconnectctl show-device $MCONNECT_DEVICE)

IFS=$'\n'

lines=($device_status)
IFS=": "
read -ra connected <<< ${lines[8]}
connected=${connected[1]}

if [ ! "$connected" = true ] ; then
  echo "^c#EBCB8B^ ^d^"
  exit 0
fi

battery_status=$(mconnectctl show-battery $MCONNECT_DEVICE)

IFS=$'\n'

lines=($battery_status)
IFS=": "
read -ra level <<< ${lines[0]}
level=${level[1]}
read -ra charging <<< ${lines[1]}
charging=${charging[1]}

if [ "$charging" = 1 ] ; then
  echo "^c#EBCB8B^ ^d^ $level%+"
else
  echo "^c#EBCB8B^ ^d^ $level%"
fi
